**Cold air curtain**

**SIGA 90/120/150C**

**Natural protection**



**Function:**

* All-metal housing, advanced fire resistance, simple installation and easy cleaning
* Optimized fan wheel with large air volume and low noise
* Applied rigid fiberglass plastic fan wheel and also quality aluminum alloy fan wheel which is specially suitable for the environment with heavy oily smoke
* Adopting optimize motor, dependable performance, motor operates 5000 hours continuously without any defects
* Flexible control methods: switch button control, remote control and automatic-door induction control
* Elegant, generous appearance design

**Technical data:**

|  |  |  |  |
| --- | --- | --- | --- |
|  | SIGA 90C | SIGA 120C | SIGA 150C |
| Rated voltage (V) | 230 | 230 | 230 |
| Rated frequency (HZ) | 50/60 | 50/60 | 50/60 |
| Installation height (m) | 2,3 ~ 3,5 | 2,3 ~ 3,5 | 2,3 ~ 3,5 |
| Input power (high/low) (W) | 150/120 | 220/170 | 265/210 |
| Rated current (A) | 0,71 | 1,04 | 1,25 |
| Air speed (m/s) | 12 | 12 | 12 |
| Air flow rate (m3/h) | 2250 | 3000 | 3800 |
| Noise (dB) | 57 | 59 | 62 |
| Dimension (mm) | 900x221x183 | 1200x221x183 | 1500x221x183 |
| Net weight (kg) | 12,7 | 15,3 | 18,6 |



***Warranty: 2 years***